HW6 Challenge Lab 6-1

**Original Network address:** 192.168.10.0/24

**Number of subnets:** 256

**Subnet mask:** 255.255.255.0

**Number of subnets needed:** 2

|  |  |
| --- | --- |
| **Network Number in CIDR** | **Host Address Range** |
| 192.168.10.0 | 126 |
| 192.168.10.128 | 126 |
|  |  |
|  |  |
|  |  |
|  |  |